fbBuild 0.20
============

Introduction:
=============
    Sad to hear the rumor of ikari stepping down, and even sadder to hear
    of the profiteers taking advantage of this... we bring you a tribute
    to ikari. If you paid for this, get a refund!

    fbBuild is a NAND image builder made to suit freeBoot style images,
    the included patches and freboot.bin core are based on the original
    works done by ikari.

    It is suitable to build rebooter images for all current JTAG exploit
    compatible xbox 360's. As with ibuild produced images, this version
    only requires a single flash 16MiB in size or larger.

What's New:
===========
    - now encrypts crl, dae, secdata, and extended binaries
        (note, odd.bin encryption not supported - as of 12611 it's obsolete)
    - metadata no longer needed (including security files)
    - improved checks
    - scriptable file lists for image build, supports multiple versions
    - minor updates and fixes

Current Limitations:
====================
    - STAY THE HELL OFF LIVE! Nuff said, we're not you're mum.

How To Use:
===========
    - See individual folders for lists of files to provide
    - if desired provide replacement cpu and 1bl keys in text files
    - open a command window in the fbBuild directory
    - on the command line type, for example:

    example - if you provided keys in appropriate text files

        fbbuild.exe -c falcon -d myfalcon myfalconout.bin

        -c falcon = use falcon bl and patch set
        -d myfalcon = a folder is present called "myfalcon" with per machine
            files
        myfalconout.bin = the file that will be produced

    - type fbbuild.exe -? for command line info

Note:
=====
    - for those of you using donor data, the security files shouldn't pose a
    problem but make sure the CPU key you use is from the machine that donated
    the kv instead of the target machine you are building the image for.

    - if you have a 16M jasper, an additional build type has been added
    'jaspersb', by default the image will be built for jasper with big block
    controller (config 00023010), use this alternate switch to build for small
    block controller (config 01198010)

Credits:
========
    Without ikari this would not have been possible, thanks!
          __               ____   ___   ___ _____
         / _|_ __ ___  ___| __ ) / _ \ / _ \_   _|
        | |_| '__/ _ \/ _ \  _ \| | | | | | || |
        |  _| | |  __/  __/ |_) | |_| | |_| || |
        |_| |_|  \___|\___|____/ \___/ \___/ |_|
                     [v0.04 - inspired by ikari]
        R.I.P.

    Thanks and greetz to everyone who has contributed to hacking this
    wonderful machine. Thanks to the engineers and countless others who made
    the machine what it is... we only wish they had listened and RROD was
    not a problem. If we were to list everyone here, there would be no time
    left to play on the machine!

    Big thanks to the folks at #freeboot on efnet for the tireless
    hours of help you all give freely. Big thanks to the testers who made
    sure stuff worked.

    Don't believe what random people *cough* write on forums ..

-----
2010/12/13
-----

Changes:
========
0.2
- scriptable file lists
- no longer any need for .meta files
- encrypts crl/secdata/dae/extended (no .meta needed)
- fixed random byte generator (yes, it was a bug)
- better checks for hacked SMC and encrypted security files

0.11
- add "jasper16a" LBA method as default for jasper
- add SMC check for encrypted and known hack SMC
- search for valid smc_config hash instead of hard coded
    offsets, support filename "config.bin"
- refine KV encryption check
- disable extended DVD auth for OSIG keyvaults (aka: AP25)
- random non-critical changes
