================ INSTRUCTIONS ==================
1. Find COM port of TTL adapter via Device Manager
2. Open auth_test.exe
3. Select COM port
4. Select Syscom Variant
5. Press Start
6. Plug adapter in and turn PS3 stanby power on
7. Click "Auth" button to gain authorisation
 - Authorisation may not work first time
 - Common errors may include the following:
   - "Program Error": This means the program recieved no response from Syscon
   - "Auth1 response invalid": This means authorisation failed
 - Continue to next step when program says "Auth Successful"
8. Press "Get Error Codes" Button
 - This may take a while
 - Program will display current process out of 20
 - Inbetween grabbing codes the program may show as "Not Responding" but the program is still working
 - An Error code may take longer to grab if Syscon is unable to complete request.
9. The program will automatically open a text file with the Error codes displayed
10. Done
================================================
================ COMPATABILITY =================
This will only work on Windows 10
Python does not need to be install on computer
================================================
=============== TROUBLESHOOTING ================
If "Unicode Error" is displayed, you will need to close program and reopen
If Dialog box pops up saying "Fetal error" you will need to reopen the program
If "Program Error" is displayed more than 5 times in a row, you need to do the following steps:
1. Close Program
2. Go to Task Manager
3. Locate uart_script.exe and end task
4. Restart Program
================================================
=================== CREDITS ====================
Original Creators: We can thank guys like 'Major' and 'zecoxao' for making this possible in the first place. We are just running their script. as well as db260179  
GUI Creator: Callum Duddle, Postal_Dude_
================================================









